Name: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Date: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**Donning SCBA Using the Over-the-Head Method Checklist**

|  |  |  |  |
| --- | --- | --- | --- |
|  | **Task steps** | **1 pt.** |  |
|  | **each** |  |
|  |  |  |
|  |  |  |  |

Position the SCBA with the valve end of the cylinder away from your body

Open the cylinder valve fully and acknowledge that the low-air alarm and the PASS device are activated

Check the cylinder and the remote gauge pressures and verbalize “within 100 psi” or “both gauges same pressure”

Raise the SCBA overhead while guiding your elbows into the loops formed by the shoulder straps

Release the harness assembly and allow the SCBA to slide down your back

Fasten the chest strap, buckle the waist strap, and adjust the shoulder straps

Don the facepiece and check the facepiece seal

Connect the air supply to the facepiece

Activate the PASS device if it is not integrated into the system

Don the hood, helmet, and gloves

**Total points (10 possible pts.)**

Comments: