Name: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Date: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**Donning SCBA Using the Seat-Mounted Method Checklist**

|  |  |  |  |
| --- | --- | --- | --- |
|  | **Task steps** | **1 pt.** |  |
|  | **each** |  |
|  |  |  |
|  |  |  |  |

Open the cylinder valve fully and acknowledge that the low-air alarm and the PASS device are activated

Check the cylinder and remote gauge pressures and verbalizes “within 100 psi” or “both gauges same pressure”

Position your body in the seat with your back firmly against the SCBA and release the SCBA hold-down device

Insert your arms through the shoulder straps

Fasten the chest strap, buckle the waist strap, and adjust the shoulder straps

Fastens your seat belt before the apparatus moves

Don the facepiece and check the facepiece seal

Connect the air supply to the facepiece when you are ready to use it

Activate the PASS device if it is not integrated into the system

Don the hood, helmet, and gloves

**Total points (10 possible pts.)**

Comments: