Name \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Date \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**Fire Hose Skills Quiz**

1. \_\_\_\_\_\_Which of the following is NOT one of the types of lugs found on fire hose couplings?
	1. Recessed
	2. Pin
	3. Storz
	4. Rocker
2. \_\_\_\_\_\_Which of the following is a hose clamp used to stop the flow of water in a hose?
	1. Screw-down
	2. Press-down
	3. Hydraulic press
	4. All are hose clamps
3. \_\_\_\_\_\_Which of the following is the simplest of all hose rolls and starts at one end—usually the male coupling?
	1. Donut Roll
	2. Straight Roll
	3. Double-donut Roll
	4. Self-locking Roll
4. \_\_\_\_\_\_Which of the following is the term most commonly used to describe the hose compartment on a fire apparatus?
	1. Hose mount
	2. Hose load
	3. Hose-bed
	4. Hose make-up
5. \_\_\_\_\_\_Which of the following is NOT a hose load?
	1. Dutchman
	2. Accordion
	3. Horseshoe
	4. Flat
6. \_\_\_\_\_\_NFPA 1500 does permit the loading of hose onto a moving apparatus as long as certain criterion are met and a local written policy is in place.
7. True
8. False
9. \_\_\_\_\_\_Which of the following is NOT included in pre-connected hose loads for attack lines?
	1. Minuteman
	2. Flat load
	3. Triple layer
	4. Tailboard
10. \_\_\_\_\_\_Which of the following are rubber-covered hoses that are usually carried pre-connected and coiled on reels?
	1. Woven jacket lines
	2. Booster lines
	3. Hard suction lines
	4. Intake lines
11. \_\_\_\_\_\_When you uncouple a hose using the Knee-Press Method, you grasp the hose behind the male coupling and stand the female coupling on end.
	1. True
	2. False
12. \_\_\_\_\_\_The first step for advancing a line into a structure is always “confirm order with officer to advance a line into the structure.
	1. True
	2. False