Name \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Date \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**Fire Hose Skills Quiz**

1. \_\_\_\_\_\_Which of the following is NOT one of the types of lugs found on fire hose couplings?
   1. Recessed
   2. Pin
   3. Storz
   4. Rocker
2. \_\_\_\_\_\_Which of the following is a hose clamp used to stop the flow of water in a hose?
   1. Screw-down
   2. Press-down
   3. Hydraulic press
   4. All are hose clamps
3. \_\_\_\_\_\_Which of the following is the simplest of all hose rolls and starts at one end—usually the male coupling?
   1. Donut Roll
   2. Straight Roll
   3. Double-donut Roll
   4. Self-locking Roll
4. \_\_\_\_\_\_Which of the following is the term most commonly used to describe the hose compartment on a fire apparatus?
   1. Hose mount
   2. Hose load
   3. Hose-bed
   4. Hose make-up
5. \_\_\_\_\_\_Which of the following is NOT a hose load?
   1. Dutchman
   2. Accordion
   3. Horseshoe
   4. Flat
6. \_\_\_\_\_\_NFPA 1500 does permit the loading of hose onto a moving apparatus as long as certain criterion are met and a local written policy is in place.
7. True
8. False
9. \_\_\_\_\_\_Which of the following is NOT included in pre-connected hose loads for attack lines?
   1. Minuteman
   2. Flat load
   3. Triple layer
   4. Tailboard
10. \_\_\_\_\_\_Which of the following are rubber-covered hoses that are usually carried pre-connected and coiled on reels?
    1. Woven jacket lines
    2. Booster lines
    3. Hard suction lines
    4. Intake lines
11. \_\_\_\_\_\_When you uncouple a hose using the Knee-Press Method, you grasp the hose behind the male coupling and stand the female coupling on end.
    1. True
    2. False
12. \_\_\_\_\_\_The first step for advancing a line into a structure is always “confirm order with officer to advance a line into the structure.
    1. True
    2. False