Name\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Date\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**Forcible Entry Tools Quiz**

1. \_\_\_\_\_ Bolt cutters can be used on which of the following?

a. Bolts

b. Chains

c. Lock hasps

d. All of the above

2. \_\_\_\_\_ Bolt cutters are not effective on

a. Lock hasps

b. Case hardened steel

c. Padlocks

d. All of the above

3. \_\_\_\_\_ Which of the following is an exothermic forcible entry tool?

a. Burning bar

b. Rebar cutter

c. Hydraulic spreader

d. Power saws

4. \_\_\_\_\_ Which of the following has a short blade that moves in and out?

a. Rotary saw

b. Skill saw

c. Reciprocating saw

d. Penetrating saw

5. \_\_\_\_\_ Which saw was originally designed for construction use?

a. Rotary saw

b. Circular saw

c. Skill saw

d. Chain saw

6. \_\_\_\_\_ Pike poles have a very limited use in forcible entry activities.

a. True

b. False

7. \_\_\_\_\_ Which of the following is commonly referred to as a “set of irons”?

a. Pick-head axe and a ram bar

b. Flat-head axe and Kelly Bar

c. Hooligan bar and an A Tool

d. Halligan bar and a flat-head axe

8. \_\_\_\_\_ Spreaders used for vehicle extrication can spread up to \_\_\_\_ inches.

a. 24

b. 32

c. 42

d. 48

9. \_\_\_\_\_ Hydraulic ram bars have a spread from \_\_\_\_ to\_\_\_\_ inches.

a. 12 to 24

b. 24 to 30

c. 30 to 48

d. 36 to 63

10. \_\_\_\_\_ Oxyacetylene cutting torches

a. Have a flame temperature of 5,700 degrees F

b. Use an unstable gas

c. Must be kept in an upright position

d. All of the above